RYK25004

|  |  |
| --- | --- |
| Color Camera | |
| Image Device | 1/3” Color CCD  Super HAD II  (Sony Chipset) effioA |
| Picture Elements | NTSC: 976x494  PAL: 976x582 |
| Resolution | 800TVL |
| Min. Illumination | 0.01 Lux/ F1.2 |
| S/N Ratio | More than 50 dB |
| Electronic Shutter | NTSC:1/60~1/100,000, PAL:1/50~1/110,000 |
| Gamma | 0.45 |
| Lens Furnished | 3.7mm lens |
| White Balance | Auto |
| Gain Control | Auto |
| Sync System | Internal |
| Video Output | 1 Vp-p/ 75 Ohms |
| Audio Output | 2 Vp-p / 50 Ohms (optional) |
| Power Supply | DC 12V ±10％ |
| Power Consumption | 175mA |
| Operating Temp. | -10 to 50℃ |